BJ60S

BiJie Meeting Box Specifications

# Appearance



# Features

* Support QR mirror and Short Code mirror
* Support 2 display of wireless projection
* Support wireless projection from Android、iOS、Mac、Windows
* Support AirPlay/Miracast/WiDi/BJCast
* 2.4G+5G dual-frequency wifi mode
* 4K HD display
* Provide AP hotspot
* Provide wireless projection SDK
* Support unified platform of management

# Specification

|  |  |  |
| --- | --- | --- |
| **items** | | **Specifications** |
|  | Operate system | Android |
| WiFi module | 802.11AC\*2 module |
| WiFi AP | AP hot |
| Network | Support wired, wireless, 802.1x |
| LED light | White LED |
| USB interface | 1 \* USB3.0 1\*USB2.0 |
| Video output | HDMI \*1 |
| Audio output | 3.5mm audio port |
| WIFI antenna | Built in high performance wifi antenna |
| Boot time | ＜30s |
| Power | DC5V2A |
| Size | 127\*97\*20mm |
| Wireless Projection  Functions | Airplay | Support Apple’s iOS、MacOS devices’ Airplay、no need to install any app  Support airplay multi-display(Present multiple screens at the same time) |
| Miracast | Support Android devices（phone、Pad）、no need to install any app support Miracast multi-display(Present multiple screens at the same time) |
| WiDi | Support Windows8/10、no need to install any app  Support WiDi multi-display(Present multiple screens at the same time) |
| BJCast | Support windows, MAC, Android, IOS device installation software client mode for wireless projection  Provide Android, IOS, MacOS, windows 4 sets of transmitter software |
| USB transmitter | Support Windows / Mac computer plug-in USB transmitter screen projection, provide visitors screen projection solution |
| Number of multi-display | 2 |
| Reverse Control | Support BJCast、USB transmitter、Miracast、WiDi |
| QR for projection | Support scanning QR code |
| Short code for projection | Support direct input of screen projection code |
| Delay of projection | ≤200ms |
| Distance of projection | 30m |
| PIN of projection | Support screen casting security encryption, compatible with miracast pin code function |
| Wallpaper | Custom replacement and wallpaper automatic update plan |
| Customize device name | support |
| language | Simplified Chinese, traditional Chinese, English, |
| Unified management platform | Support |
| SDK | Provide wireless screen projection SDK and support third-party integrated development |
| Warranty | | One year |